Network Lab 1 - Report

13302010080 Yang Liu

1. Design Details

Just a TCP over TCP proxy. Nothing extraordinary.

1. Compiling

On Windows, use Release compiling mode, with Boost library installed in E:\Libraries\. This is designed on Windows, but it should be able to run on any platform.

1. Usage

To run Alice, use:

*Server.exe 127.0.0.1 7000 172.19.0.1 8000 Alice*

To run Bob, use:

*Server.exe 172.20.0.1 8000 172.20.0.2 7000*

The Bob program will automatically redirect data flow to 127.0.0.1:8000.

1. Performance

On my computer, it can achieve 70Mbps with iperf test. Sanity test is not available for me, since I figure out Cygwin changed every LF to CRLF using pipe forwarding, and causes diff check always fails. Notepad++ text comparing shows the transferred files are the same. Forwarding traffic to a Shadowsocks client also shows completely no problem accessing websites like taobao.com:443.

Test data is shown below.

[ 4] 0.0-79.7 sec 665 MBytes 70.0 Mbits/sec

[ 4] local 172.20.0.1 port 30001 connected with 172.20.0.1 port 12929

[ 4] 0.0-25.2 sec 209 MBytes 69.7 Mbits/sec